(footprint "SMA_Samtec_SMA-J-P-H-ST-EM1_EdgeMount"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Connector SMA, 0Hz to 20GHz, 50Ohm, Edge Mount (http://suddendocs.samtec.com/prints/sma-j-p-x-st-em1-mkt.pdf)")
	(tags "SMA Straight Samtec Edge Mount")
	(property "Reference" "REF**"
		(at 0 -5.08 180)
		(layer "F.SilkS")
	)
	(property "Value" "SMA_Samtec_SMA-J-P-H-ST-EM1_EdgeMount"
		(at 0 7.62 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 90)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 90)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at 2.6 0 90)
		(layer "Dwgs.User")
	)
	(fp_text user "Board Thickness: 1.57mm"
		(at 0 5.08 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at 0 0 90)
		(size 1.27 3.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1968503937)
	)
	(pad "2" smd roundrect
		(at -0.25 -2.825 90)
		(size 1.35 3.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1851851852)
	)
	(pad "2" smd roundrect
		(at -0.25 -2.825 90)
		(size 1.35 3.7)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.1851851852)
	)
	(pad "2" smd roundrect
		(at -0.25 2.825 90)
		(size 1.35 3.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1851851852)
	)
	(pad "2" smd roundrect
		(at -0.25 2.825 90)
		(size 1.35 3.7)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.1851851852)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Samtec_SMA-J-P-H-ST-EM1_EdgeMount.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
