(footprint "SMA_Wurth_60312102114405_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Würth WR-SMA PCB SMT Jack, Vertical (https://www.we-online.com/components/products/datasheet/60312102114405.pdf)")
	(tags "Coaxial Connector 50 ohms Female")
	(property "Reference" "REF**"
		(at -1.4 -4.2 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "SMA_Wurth_60312102114405_Vertical"
		(at 0 4.8 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd circle
		(at 0 0 270)
		(size 1.73 1.73)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd custom
		(at 0 -2.8 90)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -1.595 1.6523) (xy -1.595 3.56) (xy 0.755 3.56) (xy 0.755 -3.56) (xy -1.595 -3.56) (xy -1.595 -1.6523)
					(xy -1.47693 -1.562945) (xy -1.26536 -1.355798) (xy -1.085876 -1.120305) (xy -0.94223 -0.861389)
					(xy -0.837425 -0.584464) (xy -0.773653 -0.295319) (xy -0.752246 0) (xy -0.773653 0.295319) (xy -0.837425 0.584464)
					(xy -0.94223 0.861389) (xy -1.085876 1.120305) (xy -1.26536 1.355798) (xy -1.47693 1.562945)
				)
				(width 0.001)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at 0 2.8 270)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.837425 0.584464) (xy -0.94223 0.861389) (xy -1.085876 1.120305) (xy -1.26536 1.355798) (xy -1.47693 1.562945)
					(xy -1.595 1.6523) (xy -1.595 3.56) (xy 0.755 3.56) (xy 0.755 -3.56) (xy -1.595 -3.56) (xy -1.595 -1.6523)
					(xy -1.47693 -1.562945) (xy -1.26536 -1.355798) (xy -1.085876 -1.120305) (xy -0.94223 -0.861389)
					(xy -0.837425 -0.584464) (xy -0.773653 -0.295319) (xy -0.752246 0) (xy -0.773653 0.295319)
				)
				(width 0.001)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Wurth_60312102114405_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
