(footprint "WR-MMCX_Wuerth_66011102111302_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Würth WR-MMCX PCB SMT Jack, Horizontal (https://www.we-online.com/components/products/datasheet/66011102111302.pdf)")
	(tags "Coaxial Connector 50 ohms Female")
	(property "Reference" "REF**"
		(at 0 -2.75 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "WR-MMCX_Wuerth_66011102111302_Horizontal"
		(at 0 6.05 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -1.6 -1.6 270)
		(size 0.5 0.5)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.5 -1.05) (xy -0.5 0.5) (xy 1.05 0.5) (xy 1.05 -0.645) (xy 0.995 -0.68) (xy 0.94 -0.72) (xy 0.895 -0.755)
					(xy 0.845 -0.8) (xy 0.785 -0.86) (xy 0.735 -0.92) (xy 0.68 -0.995) (xy 0.65 -1.045) (xy 0.645 -1.05)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -1.6 1.6)
		(size 0.5 0.5)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.5 -1.05) (xy -0.5 0.5) (xy 1.05 0.5) (xy 1.05 -0.645) (xy 0.995 -0.68) (xy 0.94 -0.72) (xy 0.895 -0.755)
					(xy 0.845 -0.8) (xy 0.785 -0.86) (xy 0.735 -0.92) (xy 0.68 -0.995) (xy 0.65 -1.045) (xy 0.645 -1.05)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 1.6 -1.6 180)
		(size 0.5 0.5)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.5 -1.05) (xy -0.5 0.5) (xy 1.05 0.5) (xy 1.05 -0.645) (xy 0.995 -0.68) (xy 0.94 -0.72) (xy 0.895 -0.755)
					(xy 0.845 -0.8) (xy 0.785 -0.86) (xy 0.735 -0.92) (xy 0.68 -0.995) (xy 0.65 -1.045) (xy 0.645 -1.05)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 1.6 1.6 90)
		(size 0.5 0.5)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.5 -1.05) (xy -0.5 0.5) (xy 1.05 0.5) (xy 1.05 -0.645) (xy 0.995 -0.68) (xy 0.94 -0.72) (xy 0.895 -0.755)
					(xy 0.845 -0.8) (xy 0.785 -0.86) (xy 0.735 -0.92) (xy 0.68 -0.995) (xy 0.65 -1.045) (xy 0.645 -1.05)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "1" smd circle
		(at 0 0)
		(size 1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd custom
		(at -1.6 0)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.05 -0.955) (xy 1.05 -2.1) (xy -0.5 -2.1) (xy -0.5 2.1) (xy 1.05 2.1) (xy 1.05 0.955) (xy 0.995 0.92)
					(xy 0.94 0.88) (xy 0.895 0.845) (xy 0.845 0.8) (xy 0.785 0.74) (xy 0.735 0.68) (xy 0.68 0.605)
					(xy 0.65 0.555) (xy 0.605 0.47) (xy 0.575 0.4) (xy 0.545 0.315) (xy 0.53 0.255) (xy 0.515 0.18)
					(xy 0.505 0.11) (xy 0.5 0.03) (xy 0.5 -0.03) (xy 0.505 -0.11) (xy 0.515 -0.18) (xy 0.53 -0.255)
					(xy 0.55 -0.33) (xy 0.575 -0.4) (xy 0.61 -0.48) (xy 0.635 -0.53) (xy 0.665 -0.58) (xy 0.705 -0.64)
					(xy 0.735 -0.68) (xy 0.76 -0.71) (xy 0.795 -0.75) (xy 0.84 -0.795) (xy 0.89 -0.84) (xy 0.94 -0.88)
					(xy 0.975 -0.905) (xy 1.02 -0.935)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at 1.6 0 180)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.05 -0.955) (xy 1.05 -2.1) (xy -0.5 -2.1) (xy -0.5 2.1) (xy 1.05 2.1) (xy 1.05 0.955) (xy 0.995 0.92)
					(xy 0.94 0.88) (xy 0.895 0.845) (xy 0.845 0.8) (xy 0.785 0.74) (xy 0.735 0.68) (xy 0.68 0.605)
					(xy 0.65 0.555) (xy 0.605 0.47) (xy 0.575 0.4) (xy 0.545 0.315) (xy 0.53 0.255) (xy 0.515 0.18)
					(xy 0.505 0.11) (xy 0.5 0.03) (xy 0.5 -0.03) (xy 0.505 -0.11) (xy 0.515 -0.18) (xy 0.53 -0.255)
					(xy 0.55 -0.33) (xy 0.575 -0.4) (xy 0.61 -0.48) (xy 0.635 -0.53) (xy 0.665 -0.58) (xy 0.705 -0.64)
					(xy 0.735 -0.68) (xy 0.76 -0.71) (xy 0.795 -0.75) (xy 0.84 -0.795) (xy 0.89 -0.84) (xy 0.94 -0.88)
					(xy 0.975 -0.905) (xy 1.02 -0.935)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/WR-MMCX_Wuerth_66011102111302_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
