(footprint "DIN41612_B_2x16_Male_Horizontal_THT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DIN41612 connector, type B, Horizontal, 2 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf")
	(tags "DIN 41612 IEC 60603 B")
	(property "Reference" "REF**"
		(at -5.08 1 0)
		(layer "F.SilkS")
	)
	(property "Value" "DIN41612_B_2x16_Male_Horizontal_THT"
		(at 39.37 5.08 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "Board edge"
		(at 39.37 -7.3 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 39.37 -2.54 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -5.08 -2.54)
		(size 2.85 2.85)
		(drill 2.85)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 83.82 -2.54)
		(size 2.85 2.85)
		(drill 2.85)
		(layers "*.Cu" "*.Mask")
	)
	(pad "a2" thru_hole roundrect
		(at 2.54 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.16129)
	)
	(pad "a4" thru_hole circle
		(at 7.62 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a6" thru_hole circle
		(at 12.7 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a8" thru_hole circle
		(at 17.78 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a10" thru_hole circle
		(at 22.86 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a12" thru_hole circle
		(at 27.94 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a14" thru_hole circle
		(at 33.02 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a16" thru_hole circle
		(at 38.1 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a18" thru_hole circle
		(at 43.18 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a20" thru_hole circle
		(at 48.26 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a22" thru_hole circle
		(at 53.34 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a24" thru_hole circle
		(at 58.42 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a26" thru_hole circle
		(at 63.5 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a28" thru_hole circle
		(at 68.58 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a30" thru_hole circle
		(at 73.66 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a32" thru_hole circle
		(at 78.74 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b2" thru_hole circle
		(at 2.54 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b4" thru_hole circle
		(at 7.62 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b6" thru_hole circle
		(at 12.7 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b8" thru_hole circle
		(at 17.78 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b10" thru_hole circle
		(at 22.86 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b12" thru_hole circle
		(at 27.94 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b14" thru_hole circle
		(at 33.02 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b16" thru_hole circle
		(at 38.1 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b18" thru_hole circle
		(at 43.18 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b20" thru_hole circle
		(at 48.26 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b22" thru_hole circle
		(at 53.34 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b24" thru_hole circle
		(at 58.42 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b26" thru_hole circle
		(at 63.5 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b28" thru_hole circle
		(at 68.58 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b30" thru_hole circle
		(at 73.66 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b32" thru_hole circle
		(at 78.74 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_DIN.3dshapes/DIN41612_B_2x16_Male_Horizontal_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
