(footprint "DIN41612_E_2x16_Female_Vertical_THT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DIN41612 connector, type E, Vertical, 5 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf")
	(tags "DIN 41612 IEC 60603 E")
	(property "Reference" "REF**"
		(at 5.08 -9.13 0)
		(layer "F.SilkS")
	)
	(property "Value" "DIN41612_E_2x16_Female_Vertical_THT"
		(at 5.08 87.87 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5.08 39.37 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 2.24 -5.63)
		(size 2.85 2.85)
		(drill 2.85)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.24 84.37)
		(size 2.85 2.85)
		(drill 2.85)
		(layers "*.Cu" "*.Mask")
	)
	(pad "a2" thru_hole roundrect
		(at 0 2.54)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.096154)
	)
	(pad "a4" thru_hole circle
		(at 0 7.62)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a6" thru_hole circle
		(at 0 12.7)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a8" thru_hole circle
		(at 0 17.78)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a10" thru_hole circle
		(at 0 22.86)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a12" thru_hole circle
		(at 0 27.94)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a14" thru_hole circle
		(at 0 33.02)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a16" thru_hole circle
		(at 0 38.1)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a18" thru_hole circle
		(at 0 43.18)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a20" thru_hole circle
		(at 0 48.26)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a22" thru_hole circle
		(at 0 53.34)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a24" thru_hole circle
		(at 0 58.42)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a26" thru_hole circle
		(at 0 63.5)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a28" thru_hole circle
		(at 0 68.58)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a30" thru_hole circle
		(at 0 73.66)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a32" thru_hole circle
		(at 0 78.74)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "e2" thru_hole circle
		(at 10.16 2.54)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "e4" thru_hole circle
		(at 10.16 7.62)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "e6" thru_hole circle
		(at 10.16 12.7)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "e8" thru_hole circle
		(at 10.16 17.78)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "e10" thru_hole circle
		(at 10.16 22.86)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "e12" thru_hole circle
		(at 10.16 27.94)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "e14" thru_hole circle
		(at 10.16 33.02)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "e16" thru_hole circle
		(at 10.16 38.1)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "e18" thru_hole circle
		(at 10.16 43.18)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "e20" thru_hole circle
		(at 10.16 48.26)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "e22" thru_hole circle
		(at 10.16 53.34)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "e24" thru_hole circle
		(at 10.16 58.42)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "e26" thru_hole circle
		(at 10.16 63.5)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "e28" thru_hole circle
		(at 10.16 68.58)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "e30" thru_hole circle
		(at 10.16 73.66)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "e32" thru_hole circle
		(at 10.16 78.74)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_DIN.3dshapes/DIN41612_E_2x16_Female_Vertical_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
