(footprint "DIN41612_Q3_2x10_Female_Horizontal_THT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DIN41612 connector, type Q/3, Horizontal, 2 rows 10 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf")
	(tags "DIN 41612 IEC 60603 Q/3")
	(property "Reference" "REF**"
		(at -5.08 0.86 0)
		(layer "F.SilkS")
	)
	(property "Value" "DIN41612_Q3_2x10_Female_Horizontal_THT"
		(at 11.43 5.08 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "Board edge"
		(at 11.43 -7.3 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 11.43 -2.54 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -5.08 -2.54)
		(size 2.85 2.85)
		(drill 2.85)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 27.94 -2.54)
		(size 2.85 2.85)
		(drill 2.85)
		(layers "*.Cu" "*.Mask")
	)
	(pad "a1" thru_hole roundrect
		(at 0 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.16129)
	)
	(pad "a2" thru_hole circle
		(at 2.54 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a3" thru_hole circle
		(at 5.08 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a4" thru_hole circle
		(at 7.62 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a5" thru_hole circle
		(at 10.16 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a6" thru_hole circle
		(at 12.7 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a7" thru_hole circle
		(at 15.24 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a8" thru_hole circle
		(at 17.78 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a9" thru_hole circle
		(at 20.32 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a10" thru_hole circle
		(at 22.86 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b1" thru_hole circle
		(at 0 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b2" thru_hole circle
		(at 2.54 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b3" thru_hole circle
		(at 5.08 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b4" thru_hole circle
		(at 7.62 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b5" thru_hole circle
		(at 10.16 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b6" thru_hole circle
		(at 12.7 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b7" thru_hole circle
		(at 15.24 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b8" thru_hole circle
		(at 17.78 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b9" thru_hole circle
		(at 20.32 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b10" thru_hole circle
		(at 22.86 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_DIN.3dshapes/DIN41612_Q3_2x10_Female_Horizontal_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
