(footprint "DIN41612_Q_2x32_Male_Vertical_THT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DIN41612 connector, type Q, Vertical, 2 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf")
	(tags "DIN 41612 IEC 60603 Q")
	(property "Reference" "REF**"
		(at 1.27 -9.13 0)
		(layer "F.SilkS")
	)
	(property "Value" "DIN41612_Q_2x32_Male_Vertical_THT"
		(at 1.27 87.87 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1.27 39.37 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 2.24 -5.63)
		(size 2.85 2.85)
		(drill 2.85)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.24 84.37)
		(size 2.85 2.85)
		(drill 2.85)
		(layers "*.Cu" "*.Mask")
	)
	(pad "a1" thru_hole roundrect
		(at 0 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.16129)
	)
	(pad "a2" thru_hole circle
		(at 0 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a3" thru_hole circle
		(at 0 5.08)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a4" thru_hole circle
		(at 0 7.62)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a5" thru_hole circle
		(at 0 10.16)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a6" thru_hole circle
		(at 0 12.7)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a7" thru_hole circle
		(at 0 15.24)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a8" thru_hole circle
		(at 0 17.78)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a9" thru_hole circle
		(at 0 20.32)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a10" thru_hole circle
		(at 0 22.86)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a11" thru_hole circle
		(at 0 25.4)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a12" thru_hole circle
		(at 0 27.94)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a13" thru_hole circle
		(at 0 30.48)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a14" thru_hole circle
		(at 0 33.02)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a15" thru_hole circle
		(at 0 35.56)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a16" thru_hole circle
		(at 0 38.1)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a17" thru_hole circle
		(at 0 40.64)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a18" thru_hole circle
		(at 0 43.18)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a19" thru_hole circle
		(at 0 45.72)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a20" thru_hole circle
		(at 0 48.26)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a21" thru_hole circle
		(at 0 50.8)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a22" thru_hole circle
		(at 0 53.34)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a23" thru_hole circle
		(at 0 55.88)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a24" thru_hole circle
		(at 0 58.42)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a25" thru_hole circle
		(at 0 60.96)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a26" thru_hole circle
		(at 0 63.5)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a27" thru_hole circle
		(at 0 66.04)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a28" thru_hole circle
		(at 0 68.58)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a29" thru_hole circle
		(at 0 71.12)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a30" thru_hole circle
		(at 0 73.66)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a31" thru_hole circle
		(at 0 76.2)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a32" thru_hole circle
		(at 0 78.74)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b1" thru_hole circle
		(at 2.54 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b2" thru_hole circle
		(at 2.54 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b3" thru_hole circle
		(at 2.54 5.08)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b4" thru_hole circle
		(at 2.54 7.62)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b5" thru_hole circle
		(at 2.54 10.16)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b6" thru_hole circle
		(at 2.54 12.7)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b7" thru_hole circle
		(at 2.54 15.24)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b8" thru_hole circle
		(at 2.54 17.78)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b9" thru_hole circle
		(at 2.54 20.32)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b10" thru_hole circle
		(at 2.54 22.86)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b11" thru_hole circle
		(at 2.54 25.4)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b12" thru_hole circle
		(at 2.54 27.94)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b13" thru_hole circle
		(at 2.54 30.48)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b14" thru_hole circle
		(at 2.54 33.02)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b15" thru_hole circle
		(at 2.54 35.56)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b16" thru_hole circle
		(at 2.54 38.1)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b17" thru_hole circle
		(at 2.54 40.64)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b18" thru_hole circle
		(at 2.54 43.18)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b19" thru_hole circle
		(at 2.54 45.72)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b20" thru_hole circle
		(at 2.54 48.26)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b21" thru_hole circle
		(at 2.54 50.8)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b22" thru_hole circle
		(at 2.54 53.34)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b23" thru_hole circle
		(at 2.54 55.88)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b24" thru_hole circle
		(at 2.54 58.42)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b25" thru_hole circle
		(at 2.54 60.96)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b26" thru_hole circle
		(at 2.54 63.5)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b27" thru_hole circle
		(at 2.54 66.04)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b28" thru_hole circle
		(at 2.54 68.58)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b29" thru_hole circle
		(at 2.54 71.12)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b30" thru_hole circle
		(at 2.54 73.66)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b31" thru_hole circle
		(at 2.54 76.2)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b32" thru_hole circle
		(at 2.54 78.74)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_DIN.3dshapes/DIN41612_Q_2x32_Male_Vertical_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
