(footprint "DIN41612_R2_2x16_Male_Vertical_THT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DIN41612 connector, type R/2, Vertical, 3 rows 16 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf")
	(tags "DIN 41612 IEC 60603 R/2")
	(property "Reference" "REF**"
		(at 2.54 -9.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "DIN41612_R2_2x16_Male_Vertical_THT"
		(at 2.54 47.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.54 19.05 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 2.24 -5.95)
		(size 2.85 2.85)
		(drill 2.85)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.24 44.05)
		(size 2.85 2.85)
		(drill 2.85)
		(layers "*.Cu" "*.Mask")
	)
	(pad "a1" thru_hole roundrect
		(at 0 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.16129)
	)
	(pad "a2" thru_hole circle
		(at 0 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a3" thru_hole circle
		(at 0 5.08)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a4" thru_hole circle
		(at 0 7.62)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a5" thru_hole circle
		(at 0 10.16)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a6" thru_hole circle
		(at 0 12.7)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a7" thru_hole circle
		(at 0 15.24)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a8" thru_hole circle
		(at 0 17.78)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a9" thru_hole circle
		(at 0 20.32)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a10" thru_hole circle
		(at 0 22.86)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a11" thru_hole circle
		(at 0 25.4)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a12" thru_hole circle
		(at 0 27.94)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a13" thru_hole circle
		(at 0 30.48)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a14" thru_hole circle
		(at 0 33.02)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a15" thru_hole circle
		(at 0 35.56)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a16" thru_hole circle
		(at 0 38.1)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "c1" thru_hole circle
		(at 5.08 0)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "c2" thru_hole circle
		(at 5.08 2.54)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "c3" thru_hole circle
		(at 5.08 5.08)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "c4" thru_hole circle
		(at 5.08 7.62)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "c5" thru_hole circle
		(at 5.08 10.16)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "c6" thru_hole circle
		(at 5.08 12.7)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "c7" thru_hole circle
		(at 5.08 15.24)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "c8" thru_hole circle
		(at 5.08 17.78)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "c9" thru_hole circle
		(at 5.08 20.32)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "c10" thru_hole circle
		(at 5.08 22.86)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "c11" thru_hole circle
		(at 5.08 25.4)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "c12" thru_hole circle
		(at 5.08 27.94)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "c13" thru_hole circle
		(at 5.08 30.48)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "c14" thru_hole circle
		(at 5.08 33.02)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "c15" thru_hole circle
		(at 5.08 35.56)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "c16" thru_hole circle
		(at 5.08 38.1)
		(size 1.55 1.55)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_DIN.3dshapes/DIN41612_R2_2x16_Male_Vertical_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
