(footprint "DSUB-9_Pins_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, pins (male), pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see https://docs.rs-online.com/02d6/0900766b81585df2.pdf")
	(tags "9-pin D-Sub connector horizontal angled 90deg THT pins pitch 2.77x2.54mm pin-PCB-offset 9.4mm")
	(property "Reference" "REF**"
		(at 5.54 -1.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "DSUB-9_Pins_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm"
		(at 5.54 19.84 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5.54 15.34 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.77 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 5.54 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 8.31 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 11.08 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 1.385 2.54)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 4.155 2.54)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 6.925 2.54)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 9.695 2.54)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Pins_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
