(footprint "DSUB-9_Socket_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, socket (female), pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 15.98mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
	(tags "9-pin D-Sub connector horizontal angled 90deg THT socket pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 25mm mounting-hole-offset 15.98mm")
	(property "Reference" "REF**"
		(at -5.54 -2.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "DSUB-9_Socket_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm"
		(at -5.54 25.47 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -5.54 20.885 0)
		(layer "F.Fab")
	)
	(pad "0" thru_hole circle
		(at -18.04 1.42)
		(size 4 4)
		(drill 3.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "0" thru_hole circle
		(at 6.96 1.42)
		(size 4 4)
		(drill 3.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -2.77 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at -5.54 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -8.31 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -11.08 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at -1.385 2.84)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at -4.155 2.84)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at -6.925 2.84)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -9.695 2.84)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Socket_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
