(footprint "Hirose_FH26-27S-0.3SHW_2Rows-27Pins-1MP_P0.60mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Hirose 0.30mm Pitch FFC/FPC, FH26-27S-0.3SHW, 27 Circuits (https://www.hirose.com/en/product/document?clcode=&productname=&series=FH26&documenttype=Catalog&lang=en&documentid=D49355_en), generated with kicad-footprint-generator")
	(tags "connector Hirose  horizontal")
	(property "Reference" "REF**"
		(at -0.27 -6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Hirose_FH26-27S-0.3SHW_2Rows-27Pins-1MP_P0.60mm_Horizontal"
		(at -0.27 6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.75 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.4 -3.9)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.475 -3.6)
		(size 0.65 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.4 -3.3)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.475 -3)
		(size 0.65 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.4 -2.7)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.475 -2.4)
		(size 0.65 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -1.4 -2.1)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.475 -1.8)
		(size 0.65 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -1.4 -1.5)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.475 -1.2)
		(size 0.65 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -1.4 -0.9)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.475 -0.6)
		(size 0.65 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -1.4 -0.3)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1.475 0)
		(size 0.65 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -1.4 0.3)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 1.475 0.6)
		(size 0.65 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -1.4 0.9)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 1.475 1.2)
		(size 0.65 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -1.4 1.5)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 1.475 1.8)
		(size 0.65 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -1.4 2.1)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 1.475 2.4)
		(size 0.65 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -1.4 2.7)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 1.475 3)
		(size 0.65 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -1.4 3.3)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 1.475 3.6)
		(size 0.65 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -1.4 3.9)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at -1.125 -4.6)
		(size 0.95 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at -1.125 4.6)
		(size 0.95 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/Hirose_FH26-27S-0.3SHW_2Rows-27Pins-1MP_P0.60mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
