(footprint "Hirose_FH41-30S-0.5SH_1x30_1MP_1SH_P0.5mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Hirose FH41, FFC/FPC connector, FH41-30S-0.5SH, 30 Pins per row (https://www.hirose.com/fr/product/document?clcode=CL0580-2218-5-05&productname=FH41-30S-0.5SH(05)&series=FH41&documenttype=2DDrawing&lang=fr&documentid=0001001704)")
	(tags "connector Hirose FH41 horizontal")
	(property "Reference" "REF**"
		(at 0 -4.475 0)
		(layer "F.SilkS")
	)
	(property "Value" "Hirose_FH41-30S-0.5SH_1x30_1MP_1SH_P0.5mm_Horizontal"
		(at 0 4.625 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0.075 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -7.25 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -6.75 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -6.25 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -5.75 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -5.25 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -4.75 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -4.25 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -3.75 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -3.25 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -2.75 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -2.25 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -1.75 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -1.25 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -0.75 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -0.25 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 0.25 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 0.75 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 1.25 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 1.75 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 2.25 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 2.75 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 3.25 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 3.75 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 4.25 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 4.75 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 5.25 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 5.75 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 6.25 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 6.75 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 7.25 -2.975)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at -8.5 2.275)
		(size 0.4 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at 8.5 2.275)
		(size 0.4 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -6.25 2.7)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -3.75 2.7)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -1.25 2.7)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 1.25 2.7)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 3.75 2.7)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 6.25 2.7)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/Hirose_FH41-30S-0.5SH_1x30_1MP_1SH_P0.5mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
