(footprint "JAE_FF0841SA1_2Rows-41Pins_P0.40mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex JAE 0.2mm pitch, 1mm overall height FFC/FPC connector, FF0841SA1, 41 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ108178.pdf), generated with kicad-footprint-generator")
	(tags "connector JAE  top entry")
	(property "Reference" "REF**"
		(at 0.15 -6.32 0)
		(layer "F.SilkS")
	)
	(property "Value" "JAE_FF0841SA1_2Rows-41Pins_P0.40mm_Horizontal"
		(at 0.15 6.32 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 1.02 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.35 -4)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.275 -3.8)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.35 -3.6)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.275 -3.4)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.35 -3.2)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.275 -3)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -1.35 -2.8)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.275 -2.6)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -1.35 -2.4)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.275 -2.2)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -1.35 -2)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.275 -1.8)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -1.35 -1.6)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1.275 -1.4)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -1.35 -1.2)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 1.275 -1)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -1.35 -0.8)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 1.275 -0.6)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -1.35 -0.4)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 1.275 -0.2)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -1.35 0)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 1.275 0.2)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -1.35 0.4)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 1.275 0.6)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -1.35 0.8)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 1.275 1)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -1.35 1.2)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 1.275 1.4)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -1.35 1.6)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 1.275 1.8)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at -1.35 2)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 1.275 2.2)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at -1.35 2.4)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 1.275 2.6)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at -1.35 2.8)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 1.275 3)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at -1.35 3.2)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 1.275 3.4)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at -1.35 3.6)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 1.275 3.8)
		(size 0.7 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at -1.35 4)
		(size 0.55 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/JAE_FF0841SA1_2Rows-41Pins_P0.40mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
