(footprint "Molex_54548-1071_1x10-1MP_P0.5mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex FFC/FPC connector, 10 bottom-side contacts, 0.5mm pitch, 1.2mm height, https://www.molex.com/pdm_docs/sd/545481071_sd.pdf")
	(tags "FFC FPC connector")
	(property "Reference" "REF**"
		(at 0 -2.625 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_54548-1071_1x10-1MP_P0.5mm_Horizontal"
		(at 0 5.425 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 1.125 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.25 -1.025)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.75 -1.025)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.25 -1.025)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.75 -1.025)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -0.25 -1.025)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0.25 -1.025)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0.75 -1.025)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.25 -1.025)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 1.75 -1.025)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 2.25 -1.025)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at -4.525 0.875)
		(size 1.65 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at 4.525 0.875)
		(size 1.65 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/Molex_54548-1071_1x10-1MP_P0.5mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
