(footprint "Harwin_Gecko-G125-FVX0605L0X_2x03_P1.25mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Harwin Gecko Connector, 6 pins, dual row female, vertical entry, PN:G125-FVX0605L0X, https://content.harwin.com/m/60a18b02a2a99a14/original/DRG-00168-Technical-Drawing-Datasheet-G125-FVXXX05L0P-pdf.pdf")
	(tags "connector harwin gecko")
	(property "Reference" "REF**"
		(at 1.25 -3.35 0)
		(layer "F.SilkS")
	)
	(property "Value" "Harwin_Gecko-G125-FVX0605L0X_2x03_P1.25mm_Vertical"
		(at 1.25 4.45 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1.25 0.625 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.25 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2.5 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 1.25 1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 2.5 1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Harwin.3dshapes/Harwin_Gecko-G125-FVX0605L0X_2x03_P1.25mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
