(footprint "Harwin_Gecko-G125-MVX3405L0X_2x17_P1.25mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Harwin Gecko Connector, 34 pins, dual row male, vertical entry, no latches, PN:G125-MVX3405L0X, https://content.harwin.com/m/62fd8add13144f50/original/DRG-00182-Technical-Drawing-Datasheet-G125-MVXXX05LXP-pdf.pdf")
	(tags "connector harwin gecko")
	(property "Reference" "REF**"
		(at 10 -4.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "Harwin_Gecko-G125-MVX3405L0X_2x17_P1.25mm_Vertical"
		(at 10 3.35 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 10 -0.625 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.25 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2.5 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.75 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 5 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 6.25 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 7.5 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 8.75 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 10 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 11.25 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 12.5 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 13.75 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 15 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 16.25 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 17.5 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 18.75 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 20 0)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 0 -1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at 1.25 -1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at 2.5 -1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 3.75 -1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at 5 -1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole circle
		(at 6.25 -1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at 7.5 -1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 8.75 -1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "26" thru_hole circle
		(at 10 -1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole circle
		(at 11.25 -1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "28" thru_hole circle
		(at 12.5 -1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 13.75 -1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "30" thru_hole circle
		(at 15 -1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "31" thru_hole circle
		(at 16.25 -1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "32" thru_hole circle
		(at 17.5 -1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 18.75 -1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at 20 -1.25)
		(size 0.95 0.95)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Harwin.3dshapes/Harwin_Gecko-G125-MVX3405L0X_2x17_P1.25mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
