(footprint "Harwin_M20-7810545_2x05_P2.54mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Harwin Female Vertical Surface Mount Double Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-7810545, 5 Pins per row (https://cdn.harwin.com/pdfs/M20-781.pdf), generated with kicad-footprint-generator")
	(tags "connector Harwin M20 side entry")
	(property "Reference" "REF**"
		(at 0 -7.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "Harwin_M20-7810545_2x05_P2.54mm_Vertical"
		(at 0 7.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -5.65 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -1.27 -5.08)
		(size 1.02 1.02)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 -2.54)
		(size 1.02 1.02)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 0)
		(size 1.02 1.02)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 2.54)
		(size 1.02 1.02)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 5.08)
		(size 1.02 1.02)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 -3.81)
		(size 1.8 1.8)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 3.81)
		(size 1.8 1.8)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 -5.08)
		(size 1.02 1.02)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 -2.54)
		(size 1.02 1.02)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 0)
		(size 1.02 1.02)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 2.54)
		(size 1.02 1.02)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 5.08)
		(size 1.02 1.02)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -2.91 -5.08)
		(size 1.78 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.91 -2.54)
		(size 1.78 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.91 0)
		(size 1.78 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.91 2.54)
		(size 1.78 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2.91 5.08)
		(size 1.78 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.91 -5.08)
		(size 1.78 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 2.91 -2.54)
		(size 1.78 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 2.91 0)
		(size 1.78 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 2.91 2.54)
		(size 1.78 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 2.91 5.08)
		(size 1.78 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Harwin.3dshapes/Harwin_M20-7810545_2x05_P2.54mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
