(footprint "Harwin_M20-89010xx_1x10_P2.54mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89010xx, 10 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator")
	(tags "connector Harwin M20-890 horizontal")
	(property "Reference" "REF**"
		(at -0.48 -13.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "Harwin_M20-89010xx_1x10_P2.54mm_Horizontal"
		(at -0.48 13.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -0.48 0 90)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at 3.895 -11.43)
		(size 6 0.76)
		(layers "F.SilkS")
	)
	(pad "1" smd rect
		(at -5.525 -11.43)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -5.525 -8.89)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -5.525 -6.35)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -5.525 -3.81)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -5.525 -1.27)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -5.525 1.27)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -5.525 3.81)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -5.525 6.35)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -5.525 8.89)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -5.525 11.43)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Harwin.3dshapes/Harwin_M20-89010xx_1x10_P2.54mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
