(footprint "Hirose_BM24_BM24-40DS-2-0.35V_2x20_P0.35mm_PowerPin2_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Hirose BM24 series connector, BM24-40DS/2-0.35V (https://www.hirose.com/product/en/download_file/key_name/BM24/category/Catalog/doc_file_id/47680/?file_category_id=4&item_id=50&is_series=1)")
	(tags "connector Hirose 40pin receptacle vertical")
	(property "Reference" "REF**"
		(at 0 -6.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Hirose_BM24_BM24-40DS-2-0.35V_2x20_P0.35mm_PowerPin2_Vertical"
		(at 0 7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "No exposed copper"
		(at -0.5 0 90)
		(layer "Cmts.User")
	)
	(fp_text user "No exposed copper"
		(at 0.4 0 90)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0.15 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.06 -3.325 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.06 -3.325 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.06 -2.975 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.06 -2.975 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.06 -2.625 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.06 -2.625 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -1.06 -2.275 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.06 -2.275 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -1.06 -1.925 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.06 -1.925 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -1.06 -1.575 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.06 -1.575 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -1.06 -1.225 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1.06 -1.225 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -1.06 -0.875 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 1.06 -0.875 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -1.06 -0.525 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 1.06 -0.525 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -1.06 -0.175 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 1.06 -0.175 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -1.06 0.175 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 1.06 0.175 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -1.06 0.525 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 1.06 0.525 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -1.06 0.875 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 1.06 0.875 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -1.06 1.225 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 1.06 1.225 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -1.06 1.575 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 1.06 1.575 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at -1.06 1.925 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 1.06 1.925 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at -1.06 2.275 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 1.06 2.275 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at -1.06 2.625 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 1.06 2.625 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at -1.06 2.975 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 1.06 2.975 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at -1.06 3.325 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 1.06 3.325 90)
		(size 0.18 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 0 -5.155 90)
		(size 0.49 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 0 5.155 90)
		(size 0.49 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_BM24_BM24-40DS-2-0.35V_2x20_P0.35mm_PowerPin2_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
