(footprint "Hirose_DF12_DF12C3.0-10DS-0.5V_2x05_P0.50mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Hirose DF12C SMD, DF12C3.0-10DS-0.5V, 10 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0694-9-81&productname=DF12C(3.0)-50DS-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000994748), generated with kicad-footprint-generator")
	(tags "connector Hirose DF12 vertical")
	(property "Reference" "REF**"
		(at 0 -4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Hirose_DF12_DF12C3.0-10DS-0.5V_2x05_P0.50mm_Vertical"
		(at 0 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -1.1 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.5 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.5 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.5 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.5 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -1 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at -0.5 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd rect
		(at 0 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" smd rect
		(at 0.5 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "5" smd rect
		(at 1 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" smd rect
		(at -1 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "7" smd rect
		(at -0.5 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" smd rect
		(at 0 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "9" smd rect
		(at 0.5 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd rect
		(at 1 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF12_DF12C3.0-10DS-0.5V_2x05_P0.50mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
