(footprint "Hirose_DF12_DF12E3.0-60DP-0.5V_2x30_P0.50mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Hirose DF12E SMD, DF12E3.0-60DP-0.5V, 60 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0834-6-81&productname=DF12E(3.0)-50DP-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000992393), generated with kicad-footprint-generator")
	(tags "connector Hirose DF12 vertical")
	(property "Reference" "REF**"
		(at 0 -4.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "Hirose_DF12_DF12E3.0-60DP-0.5V_2x30_P0.50mm_Vertical"
		(at 0 4.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -1.2 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -7.25 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -7.25 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.75 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.75 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.25 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.25 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.75 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.75 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.25 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.25 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4.75 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4.75 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4.25 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4.25 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.75 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.75 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.25 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.25 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.75 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.75 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.25 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.25 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.75 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.75 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.25 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.25 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.75 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.75 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.25 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.25 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.25 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.25 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.75 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.75 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.25 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.25 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.75 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.75 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.25 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.25 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.75 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.75 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.25 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.25 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.75 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.75 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.25 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.25 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.75 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.75 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 5.25 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 5.25 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 5.75 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 5.75 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 6.25 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 6.25 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 6.75 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 6.75 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 7.25 -2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 7.25 2)
		(size 0.28 1.2)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -7.25 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at -6.75 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd rect
		(at -6.25 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" smd rect
		(at -5.75 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "5" smd rect
		(at -5.25 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" smd rect
		(at -4.75 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "7" smd rect
		(at -4.25 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" smd rect
		(at -3.75 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "9" smd rect
		(at -3.25 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd rect
		(at -2.75 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "11" smd rect
		(at -2.25 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" smd rect
		(at -1.75 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "13" smd rect
		(at -1.25 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" smd rect
		(at -0.75 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "15" smd rect
		(at -0.25 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" smd rect
		(at 0.25 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "17" smd rect
		(at 0.75 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "18" smd rect
		(at 1.25 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "19" smd rect
		(at 1.75 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" smd rect
		(at 2.25 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "21" smd rect
		(at 2.75 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "22" smd rect
		(at 3.25 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "23" smd rect
		(at 3.75 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" smd rect
		(at 4.25 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "25" smd rect
		(at 4.75 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "26" smd rect
		(at 5.25 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "27" smd rect
		(at 5.75 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "28" smd rect
		(at 6.25 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "29" smd rect
		(at 6.75 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "30" smd rect
		(at 7.25 1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "31" smd rect
		(at -7.25 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "32" smd rect
		(at -6.75 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "33" smd rect
		(at -6.25 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "34" smd rect
		(at -5.75 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "35" smd rect
		(at -5.25 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "36" smd rect
		(at -4.75 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "37" smd rect
		(at -4.25 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "38" smd rect
		(at -3.75 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "39" smd rect
		(at -3.25 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "40" smd rect
		(at -2.75 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "41" smd rect
		(at -2.25 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "42" smd rect
		(at -1.75 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "43" smd rect
		(at -1.25 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "44" smd rect
		(at -0.75 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "45" smd rect
		(at -0.25 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "46" smd rect
		(at 0.25 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "47" smd rect
		(at 0.75 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "48" smd rect
		(at 1.25 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "49" smd rect
		(at 1.75 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "50" smd rect
		(at 2.25 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "51" smd rect
		(at 2.75 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "52" smd rect
		(at 3.25 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "53" smd rect
		(at 3.75 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "54" smd rect
		(at 4.25 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "55" smd rect
		(at 4.75 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "56" smd rect
		(at 5.25 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "57" smd rect
		(at 5.75 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "58" smd rect
		(at 6.25 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "59" smd rect
		(at 6.75 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "60" smd rect
		(at 7.25 -1.8)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF12_DF12E3.0-60DP-0.5V_2x30_P0.50mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
