(footprint "Hirose_DF63-6P-3.96DSA_1x06_P3.96mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Hirose DF63 through hole, DF63-6P-3.96DSA, 6 Pins per row (https://www.hirose.com/product/en/products/DF63/), generated with kicad-footprint-generator")
	(tags "connector Hirose DF63 vertical")
	(property "Reference" "REF**"
		(at 9.9 -5.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "Hirose_DF63-6P-3.96DSA_1x06_P3.96mm_Vertical"
		(at 9.9 5.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 9.9 -3.75 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -1.5 3.25)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.46 2.8)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.101626)
	)
	(pad "2" thru_hole oval
		(at 3.96 0)
		(size 2.46 2.8)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 7.92 0)
		(size 2.46 2.8)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 11.88 0)
		(size 2.46 2.8)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 15.84 0)
		(size 2.46 2.8)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 19.8 0)
		(size 2.46 2.8)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF63-6P-3.96DSA_1x06_P3.96mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
