(footprint "Hirose_FX8-90P-SV_2x45_P0.6mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "0.6mm Pitch, Stacking Height 3mm to 16mm, Header, vertical (source: https://www.hirose.com/de/product/document?clcode=&productname=&series=FX8&documenttype=Catalog&lang=en&documentid=D31612_en)")
	(tags "conn hirose board to board stacking header")
	(property "Reference" "REF**"
		(at 0 -4.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "Hirose_FX8-90P-SV_2x45_P0.6mm"
		(at 0 4.65 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -15.6 1.5)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 15.6 1.5)
		(size 0.7 0.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd roundrect
		(at -13.2 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -13.2 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -12.6 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -12.6 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -12 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -12 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -11.4 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -11.4 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -10.8 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -10.8 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -10.2 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -10.2 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -9.6 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -9.6 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -9 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -9 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -8.4 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at -8.4 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -7.8 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at -7.8 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at -7.2 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at -7.2 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at -6.6 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at -6.6 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at -6 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at -6 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at -5.4 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at -5.4 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at -4.8 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at -4.8 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at -4.2 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at -4.2 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at -3.6 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at -3.6 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at -3 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at -3 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at -2.4 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at -2.4 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at -1.8 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at -1.8 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd roundrect
		(at -1.2 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "42" smd roundrect
		(at -1.2 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "43" smd roundrect
		(at -0.6 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "44" smd roundrect
		(at -0.6 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "45" smd roundrect
		(at 0 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "46" smd roundrect
		(at 0 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "47" smd roundrect
		(at 0.6 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "48" smd roundrect
		(at 0.6 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "49" smd roundrect
		(at 1.2 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "50" smd roundrect
		(at 1.2 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "51" smd roundrect
		(at 1.8 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "52" smd roundrect
		(at 1.8 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "53" smd roundrect
		(at 2.4 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "54" smd roundrect
		(at 2.4 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "55" smd roundrect
		(at 3 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "56" smd roundrect
		(at 3 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "57" smd roundrect
		(at 3.6 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "58" smd roundrect
		(at 3.6 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "59" smd roundrect
		(at 4.2 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "60" smd roundrect
		(at 4.2 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "61" smd roundrect
		(at 4.8 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "62" smd roundrect
		(at 4.8 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "63" smd roundrect
		(at 5.4 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "64" smd roundrect
		(at 5.4 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "65" smd roundrect
		(at 6 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "66" smd roundrect
		(at 6 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "67" smd roundrect
		(at 6.6 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "68" smd roundrect
		(at 6.6 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "69" smd roundrect
		(at 7.2 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "70" smd roundrect
		(at 7.2 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "71" smd roundrect
		(at 7.8 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "72" smd roundrect
		(at 7.8 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "73" smd roundrect
		(at 8.4 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "74" smd roundrect
		(at 8.4 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "75" smd roundrect
		(at 9 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "76" smd roundrect
		(at 9 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "77" smd roundrect
		(at 9.6 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "78" smd roundrect
		(at 9.6 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "79" smd roundrect
		(at 10.2 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "80" smd roundrect
		(at 10.2 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "81" smd roundrect
		(at 10.8 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "82" smd roundrect
		(at 10.8 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "83" smd roundrect
		(at 11.4 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "84" smd roundrect
		(at 11.4 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "85" smd roundrect
		(at 12 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "86" smd roundrect
		(at 12 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "87" smd roundrect
		(at 12.6 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "88" smd roundrect
		(at 12.6 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "89" smd roundrect
		(at 13.2 2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "90" smd roundrect
		(at 13.2 -2.7)
		(size 0.35 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Hirose_FX8.3dshapes/Hirose_FX8-90P-SV_2x45_P0.6mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
