(footprint "IDC-Header_2x07_P2.54mm_Horizontal_Lock"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)")
	(tags "connector idc locked")
	(property "Reference" "REF**"
		(at 12.55 8.25 90)
		(layer "F.SilkS")
	)
	(property "Value" "IDC-Header_2x07_P2.54mm_Horizontal_Lock"
		(at -2.794 6.604 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 10.16 8.255 90)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at 1.78 -5.84 90)
		(size 3.05 3.05)
		(drill 2.54)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 1.78 21.08 90)
		(size 3.05 3.05)
		(drill 2.54)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 0 90)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.54 0 90)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 2.54 90)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.54 2.54 90)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 5.08 90)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 2.54 5.08 90)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 0 7.62 90)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 2.54 7.62 90)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 0 10.16 90)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 2.54 10.16 90)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 0 12.7 90)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 2.54 12.7 90)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 0 15.24 90)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 2.54 15.24 90)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x07_P2.54mm_Horizontal_Lock.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
