(footprint "IDC-Header_2x11_P2.54mm_Vertical"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Through hole IDC box header, 2x11, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
	(tags "Through hole vertical IDC box header THT 2x11 2.54mm double row")
	(property "Reference" "REF**"
		(at 1.27 -6.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "IDC-Header_2x11_P2.54mm_Vertical"
		(at 1.27 31.5 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(roundrect_rratio 0.147059)
	)
	(pad "3" thru_hole circle
		(at 0 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "5" thru_hole circle
		(at 0 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "7" thru_hole circle
		(at 0 7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "9" thru_hole circle
		(at 0 10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "11" thru_hole circle
		(at 0 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "13" thru_hole circle
		(at 0 15.24)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "15" thru_hole circle
		(at 0 17.78)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "17" thru_hole circle
		(at 0 20.32)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "19" thru_hole circle
		(at 0 22.86)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "21" thru_hole circle
		(at 0 25.4)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "2" thru_hole circle
		(at 2.54 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "4" thru_hole circle
		(at 2.54 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "6" thru_hole circle
		(at 2.54 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "8" thru_hole circle
		(at 2.54 7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "10" thru_hole circle
		(at 2.54 10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "12" thru_hole circle
		(at 2.54 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "14" thru_hole circle
		(at 2.54 15.24)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "16" thru_hole circle
		(at 2.54 17.78)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "18" thru_hole circle
		(at 2.54 20.32)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "20" thru_hole circle
		(at 2.54 22.86)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "22" thru_hole circle
		(at 2.54 25.4)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(fp_text user "${REFERENCE}"
		(at 1.27 12.7 90)
		(layer "F.Fab")
	)
	(model "${KICAD9_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x11_P2.54mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
