(footprint "IDC-Header_2x22_P2.54mm_Horizontal"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Through hole IDC box header, 2x22, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
	(tags "Through hole horizontal IDC box header THT 2x22 2.54mm double row")
	(property "Reference" "REF**"
		(at 6.215 -6.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "IDC-Header_2x22_P2.54mm_Horizontal"
		(at 6.215 59.44 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(roundrect_rratio 0.147059)
	)
	(pad "3" thru_hole circle
		(at 0 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "5" thru_hole circle
		(at 0 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "7" thru_hole circle
		(at 0 7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "9" thru_hole circle
		(at 0 10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "11" thru_hole circle
		(at 0 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "13" thru_hole circle
		(at 0 15.24)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "15" thru_hole circle
		(at 0 17.78)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "17" thru_hole circle
		(at 0 20.32)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "19" thru_hole circle
		(at 0 22.86)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "21" thru_hole circle
		(at 0 25.4)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "23" thru_hole circle
		(at 0 27.94)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "25" thru_hole circle
		(at 0 30.48)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "27" thru_hole circle
		(at 0 33.02)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "29" thru_hole circle
		(at 0 35.56)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "31" thru_hole circle
		(at 0 38.1)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "33" thru_hole circle
		(at 0 40.64)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "35" thru_hole circle
		(at 0 43.18)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "37" thru_hole circle
		(at 0 45.72)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "39" thru_hole circle
		(at 0 48.26)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "41" thru_hole circle
		(at 0 50.8)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "43" thru_hole circle
		(at 0 53.34)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "2" thru_hole circle
		(at 2.54 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "4" thru_hole circle
		(at 2.54 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "6" thru_hole circle
		(at 2.54 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "8" thru_hole circle
		(at 2.54 7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "10" thru_hole circle
		(at 2.54 10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "12" thru_hole circle
		(at 2.54 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "14" thru_hole circle
		(at 2.54 15.24)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "16" thru_hole circle
		(at 2.54 17.78)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "18" thru_hole circle
		(at 2.54 20.32)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "20" thru_hole circle
		(at 2.54 22.86)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "22" thru_hole circle
		(at 2.54 25.4)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "24" thru_hole circle
		(at 2.54 27.94)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "26" thru_hole circle
		(at 2.54 30.48)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "28" thru_hole circle
		(at 2.54 33.02)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "30" thru_hole circle
		(at 2.54 35.56)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "32" thru_hole circle
		(at 2.54 38.1)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "34" thru_hole circle
		(at 2.54 40.64)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "36" thru_hole circle
		(at 2.54 43.18)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "38" thru_hole circle
		(at 2.54 45.72)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "40" thru_hole circle
		(at 2.54 48.26)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "42" thru_hole circle
		(at 2.54 50.8)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "44" thru_hole circle
		(at 2.54 53.34)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(fp_text user "${REFERENCE}"
		(at 8.83 26.67 90)
		(layer "F.Fab")
	)
	(model "${KICAD9_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x22_P2.54mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
