(footprint "JAE_LY20-44P-DT1_2x22_P2.00mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex LY 20 series connector, LY20-44P-DT1, 22 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator")
	(tags "connector JAE  side entry")
	(property "Reference" "REF**"
		(at 1 -3 0)
		(layer "F.SilkS")
	)
	(property "Value" "JAE_LY20-44P-DT1_2x22_P2.00mm_Vertical"
		(at 1 45 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.95 21 90)
		(layer "F.Fab")
	)
	(pad "a1" thru_hole roundrect
		(at 0 0)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.208333)
	)
	(pad "a2" thru_hole circle
		(at 0 2)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a3" thru_hole circle
		(at 0 4)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a4" thru_hole circle
		(at 0 6)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a5" thru_hole circle
		(at 0 8)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a6" thru_hole circle
		(at 0 10)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a7" thru_hole circle
		(at 0 12)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a8" thru_hole circle
		(at 0 14)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a9" thru_hole circle
		(at 0 16)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a10" thru_hole circle
		(at 0 18)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a11" thru_hole circle
		(at 0 20)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a12" thru_hole circle
		(at 0 22)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a13" thru_hole circle
		(at 0 24)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a14" thru_hole circle
		(at 0 26)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a15" thru_hole circle
		(at 0 28)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a16" thru_hole circle
		(at 0 30)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a17" thru_hole circle
		(at 0 32)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a18" thru_hole circle
		(at 0 34)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a19" thru_hole circle
		(at 0 36)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a20" thru_hole circle
		(at 0 38)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a21" thru_hole circle
		(at 0 40)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a22" thru_hole circle
		(at 0 42)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b1" thru_hole circle
		(at 2 0)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b2" thru_hole circle
		(at 2 2)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b3" thru_hole circle
		(at 2 4)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b4" thru_hole circle
		(at 2 6)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b5" thru_hole circle
		(at 2 8)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b6" thru_hole circle
		(at 2 10)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b7" thru_hole circle
		(at 2 12)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b8" thru_hole circle
		(at 2 14)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b9" thru_hole circle
		(at 2 16)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b10" thru_hole circle
		(at 2 18)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b11" thru_hole circle
		(at 2 20)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b12" thru_hole circle
		(at 2 22)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b13" thru_hole circle
		(at 2 24)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b14" thru_hole circle
		(at 2 26)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b15" thru_hole circle
		(at 2 28)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b16" thru_hole circle
		(at 2 30)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b17" thru_hole circle
		(at 2 32)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b18" thru_hole circle
		(at 2 34)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b19" thru_hole circle
		(at 2 36)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b20" thru_hole circle
		(at 2 38)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b21" thru_hole circle
		(at 2 40)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b22" thru_hole circle
		(at 2 42)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JAE.3dshapes/JAE_LY20-44P-DT1_2x22_P2.00mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
