(footprint "JAE_MM70-314-310B1"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.heilind.com/marketing/documents/jae/JAE_MM70.pdf")
	(tags "connector JAE MXM")
	(property "Reference" "REF**"
		(at 0 -7 0)
		(layer "F.SilkS")
	)
	(property "Value" "JAE_MM70-314-310B1"
		(at 0 9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 6.5 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -41 -1.1)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 41 -1.1)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -29 4.1)
		(size 2.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -29.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -29 4.1)
		(size 2.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -29.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -29 4.1)
		(size 2.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -28.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -29 4.1)
		(size 2.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -28.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -29 4.1)
		(size 2.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -27.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -26.75 4.1)
		(size 1.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -27.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -26.75 4.1)
		(size 1.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -26.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -26.75 4.1)
		(size 1.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -26.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -26.75 4.1)
		(size 1.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -25.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -25.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -25.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -25 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -24.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -24.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at -24.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -24 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at -23.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -23.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at -23.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -23 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at -22.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at -22.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at -22.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at -22 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at -21.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at -21.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at -21.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at -21 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at -20.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at -20.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at -20.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at -20 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at -19.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at -19.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at -19.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at -19 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at -18.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at -18.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at -18.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at -18 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at -17.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at -17.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at -17.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at -17 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at -16.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at -16.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at -16.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at -16 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd rect
		(at -15.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd rect
		(at -15.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd rect
		(at -15.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd rect
		(at -15 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd rect
		(at -14.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd rect
		(at -14.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd rect
		(at -14.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd rect
		(at -14 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "66" smd rect
		(at -13.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "67" smd rect
		(at -13.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "68" smd rect
		(at -13.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "69" smd rect
		(at -13 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "70" smd rect
		(at -12.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "71" smd rect
		(at -12.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "72" smd rect
		(at -12.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "73" smd rect
		(at -12 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "74" smd rect
		(at -11.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "75" smd rect
		(at -11.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "76" smd rect
		(at -11.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "77" smd rect
		(at -11 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "78" smd rect
		(at -10.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "79" smd rect
		(at -10.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "80" smd rect
		(at -10.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "81" smd rect
		(at -10 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "82" smd rect
		(at -9.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "83" smd rect
		(at -9.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "84" smd rect
		(at -9.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "85" smd rect
		(at -9 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "86" smd rect
		(at -8.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "87" smd rect
		(at -8.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "88" smd rect
		(at -8.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "89" smd rect
		(at -8 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "90" smd rect
		(at -7.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "91" smd rect
		(at -7.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "92" smd rect
		(at -7.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "93" smd rect
		(at -7 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "94" smd rect
		(at -6.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "95" smd rect
		(at -6.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "96" smd rect
		(at -6.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "97" smd rect
		(at -6 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "98" smd rect
		(at -5.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "99" smd rect
		(at -5.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "100" smd rect
		(at -5.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "101" smd rect
		(at -5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "102" smd rect
		(at -4.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "103" smd rect
		(at -4.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "104" smd rect
		(at -4.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "105" smd rect
		(at -4 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "106" smd rect
		(at -3.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "107" smd rect
		(at -3.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "108" smd rect
		(at -3.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "109" smd rect
		(at -3 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "110" smd rect
		(at -2.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "111" smd rect
		(at -2.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "112" smd rect
		(at -2.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "113" smd rect
		(at -2 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "114" smd rect
		(at -1.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "115" smd rect
		(at -1.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "116" smd rect
		(at -1.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "117" smd rect
		(at -1 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "118" smd rect
		(at -0.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "119" smd rect
		(at -0.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "120" smd rect
		(at -0.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "121" smd rect
		(at 0 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "122" smd rect
		(at 0.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "123" smd rect
		(at 0.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "124" smd rect
		(at 0.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "125" smd rect
		(at 1 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "133" smd rect
		(at 3 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "134" smd rect
		(at 3.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "135" smd rect
		(at 3.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "136" smd rect
		(at 3.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "137" smd rect
		(at 4 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "138" smd rect
		(at 4.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "139" smd rect
		(at 4.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "140" smd rect
		(at 4.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "141" smd rect
		(at 5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "142" smd rect
		(at 5.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "143" smd rect
		(at 5.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "144" smd rect
		(at 5.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "145" smd rect
		(at 6 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "146" smd rect
		(at 6.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "147" smd rect
		(at 6.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "148" smd rect
		(at 6.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "149" smd rect
		(at 7 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "150" smd rect
		(at 7.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "151" smd rect
		(at 7.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "152" smd rect
		(at 7.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "153" smd rect
		(at 8 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "154" smd rect
		(at 8.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "155" smd rect
		(at 8.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "156" smd rect
		(at 8.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "157" smd rect
		(at 9 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "158" smd rect
		(at 9.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "159" smd rect
		(at 9.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "160" smd rect
		(at 9.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "161" smd rect
		(at 10 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "162" smd rect
		(at 10.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "163" smd rect
		(at 10.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "164" smd rect
		(at 10.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "165" smd rect
		(at 11 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "166" smd rect
		(at 11.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "167" smd rect
		(at 11.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "168" smd rect
		(at 11.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "169" smd rect
		(at 12 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "170" smd rect
		(at 12.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "171" smd rect
		(at 12.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "172" smd rect
		(at 12.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "173" smd rect
		(at 13 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "174" smd rect
		(at 13.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "175" smd rect
		(at 13.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "176" smd rect
		(at 13.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "177" smd rect
		(at 14 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "178" smd rect
		(at 14.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "179" smd rect
		(at 14.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "180" smd rect
		(at 14.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "181" smd rect
		(at 15 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "182" smd rect
		(at 15.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "183" smd rect
		(at 15.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "184" smd rect
		(at 15.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "185" smd rect
		(at 16 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "186" smd rect
		(at 16.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "187" smd rect
		(at 16.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "188" smd rect
		(at 16.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "189" smd rect
		(at 17 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "190" smd rect
		(at 17.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "191" smd rect
		(at 17.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "192" smd rect
		(at 17.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "193" smd rect
		(at 18 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "194" smd rect
		(at 18.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "195" smd rect
		(at 18.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "196" smd rect
		(at 18.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "197" smd rect
		(at 19 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "198" smd rect
		(at 19.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "199" smd rect
		(at 19.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "200" smd rect
		(at 19.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "201" smd rect
		(at 20 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "202" smd rect
		(at 20.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "203" smd rect
		(at 20.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "204" smd rect
		(at 20.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "205" smd rect
		(at 21 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "206" smd rect
		(at 21.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "207" smd rect
		(at 21.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "208" smd rect
		(at 21.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "209" smd rect
		(at 22 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "210" smd rect
		(at 22.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "211" smd rect
		(at 22.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "212" smd rect
		(at 22.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "213" smd rect
		(at 23 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "214" smd rect
		(at 23.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "215" smd rect
		(at 23.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "216" smd rect
		(at 23.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "217" smd rect
		(at 24 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "218" smd rect
		(at 24.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "219" smd rect
		(at 24.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "220" smd rect
		(at 24.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "221" smd rect
		(at 25 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "222" smd rect
		(at 25.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "223" smd rect
		(at 25.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "224" smd rect
		(at 25.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "225" smd rect
		(at 26 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "226" smd rect
		(at 26.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "227" smd rect
		(at 26.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "228" smd rect
		(at 26.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "229" smd rect
		(at 27 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "230" smd rect
		(at 27.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "231" smd rect
		(at 27.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "232" smd rect
		(at 27.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "233" smd rect
		(at 28 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "234" smd rect
		(at 28.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "235" smd rect
		(at 28.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "236" smd rect
		(at 28.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "237" smd rect
		(at 29 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "238" smd rect
		(at 29.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "239" smd rect
		(at 29.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "240" smd rect
		(at 29.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "241" smd rect
		(at 30 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "242" smd rect
		(at 30.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "243" smd rect
		(at 30.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "244" smd rect
		(at 30.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "245" smd rect
		(at 31 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "246" smd rect
		(at 31.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "247" smd rect
		(at 31.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "248" smd rect
		(at 31.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "249" smd rect
		(at 32 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "250" smd rect
		(at 32.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "251" smd rect
		(at 32.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "252" smd rect
		(at 32.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "253" smd rect
		(at 33 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "254" smd rect
		(at 33.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "255" smd rect
		(at 33.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "256" smd rect
		(at 33.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "257" smd rect
		(at 34 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "258" smd rect
		(at 34.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "259" smd rect
		(at 34.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "260" smd rect
		(at 34.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "261" smd rect
		(at 35 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "262" smd rect
		(at 35.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "263" smd rect
		(at 35.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "264" smd rect
		(at 35.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "265" smd rect
		(at 36 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "266" smd rect
		(at 36.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "267" smd rect
		(at 36.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "268" smd rect
		(at 36.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "269" smd rect
		(at 37 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "270" smd rect
		(at 37.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "271" smd rect
		(at 37.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "272" smd rect
		(at 37.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "273" smd rect
		(at 38 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "274" smd rect
		(at 38.25 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "275" smd rect
		(at 38.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "276" smd rect
		(at 38.75 -4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "277" smd rect
		(at 39 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "278" smd rect
		(at 39.5 -4.1)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "279" smd rect
		(at 39.5 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "280" smd rect
		(at 39.5 -4.1)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "281" smd rect
		(at 40 4.1)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd rect
		(at -37.75 4.1)
		(size 4.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd rect
		(at -37.5 -4.1)
		(size 4.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd rect
		(at -32.75 4.1)
		(size 4.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd rect
		(at -32.5 -4.1)
		(size 4.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at -43.95 0)
		(size 3.3 5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at 43.95 0)
		(size 3.3 5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JAE.3dshapes/JAE_MM70-314-310B1.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
