(footprint "JAE_SIM_Card_SF72S006"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SIM Card, Push-Push, https://www.jae.com/direct/topics/topics_file_download/topics_id=68892&ext_no=06&index=0&_lang=en&v=202003111511468456809")
	(tags "SIM Card with Detect Switch")
	(property "Reference" "REF**"
		(at 2.667 10.541 180)
		(layer "F.SilkS")
	)
	(property "Value" "JAE_SIM_Card_SF72S006"
		(at -0.98 -6.485 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 2.54 180)
		(layer "F.Fab")
	)
	(pad "C1" smd rect
		(at -2.54 -2.46 180)
		(size 0.9 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd rect
		(at 0 -2.46 180)
		(size 0.9 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd rect
		(at 2.54 -2.46 180)
		(size 0.9 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd rect
		(at -2.54 0.71 180)
		(size 0.9 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C6" smd rect
		(at 0 0.71 180)
		(size 0.9 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C7" smd rect
		(at 2.54 0.71 180)
		(size 0.9 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "CSW" smd rect
		(at 4.27 4.04 180)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "DSW" smd rect
		(at 0.55 7.715 180)
		(size 1.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -6.555 -3.16 180)
		(size 0.45 2.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -6.555 1.69 180)
		(size 0.45 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -6.555 6.84 180)
		(size 0.45 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -2.2 8.79 180)
		(size 1.4 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -1.22 -4.31 180)
		(size 0.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 1.22 -4.31 180)
		(size 0.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 2.22 8.79 180)
		(size 1.4 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 4.095 5.84 180)
		(size 0.75 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 4.595 -3.16 180)
		(size 0.45 2.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 4.595 1.69 180)
		(size 0.45 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JAE.3dshapes/JAE_SIM_Card_SF72S006.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
