(footprint "JST_LEA_SM02B-LEASS-TF_1x02-1MP_P4.20mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "JST LEA series connector, SM02B-LEASS-TF (http://www.jst-mfg.com/product/pdf/eng/eLEA.pdf), generated with kicad-footprint-generator")
	(tags "connector JST LEA horizontal")
	(property "Reference" "REF**"
		(at 0 -4.42 0)
		(layer "F.SilkS")
	)
	(property "Value" "JST_LEA_SM02B-LEASS-TF_1x02-1MP_P4.20mm_Horizontal"
		(at 0 4.62 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.1 -2.325)
		(size 1.05 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.238095)
	)
	(pad "2" smd roundrect
		(at 2.1 -2.325)
		(size 1.05 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.238095)
	)
	(pad "MP" smd roundrect
		(at -3.675 2.35)
		(size 0.85 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP" smd roundrect
		(at 3.675 2.35)
		(size 0.85 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_LEA_SM02B-LEASS-TF_1x02-1MP_P4.20mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
