(footprint "JST_PH_B3B-PH-SM4-TB_1x03-1MP_P2.00mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "JST PH series connector, B3B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST PH vertical")
	(property "Reference" "REF**"
		(at 0 -5.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "JST_PH_B3B-PH-SM4-TB_1x03-1MP_P2.00mm_Vertical"
		(at 0 4.45 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -1 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2 0.5)
		(size 1 5.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 0 0.5)
		(size 1 5.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 2 0.5)
		(size 1 5.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP" smd roundrect
		(at -4.4 -1.75)
		(size 1.6 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
	)
	(pad "MP" smd roundrect
		(at 4.4 -1.75)
		(size 1.6 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B3B-PH-SM4-TB_1x03-1MP_P2.00mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
