(footprint "JST_PH_S12B-PH-SM4-TB_1x12-1MP_P2.00mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "JST PH series connector, S12B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST PH horizontal")
	(property "Reference" "REF**"
		(at 0 -5.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "JST_PH_S12B-PH-SM4-TB_1x12-1MP_P2.00mm_Horizontal"
		(at 0 5.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 1.5 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -11 -2.85)
		(size 1 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -9 -2.85)
		(size 1 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -7 -2.85)
		(size 1 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -5 -2.85)
		(size 1 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -3 -2.85)
		(size 1 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -1 -2.85)
		(size 1 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 1 -2.85)
		(size 1 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 3 -2.85)
		(size 1 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 5 -2.85)
		(size 1 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 7 -2.85)
		(size 1 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 9 -2.85)
		(size 1 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 11 -2.85)
		(size 1 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP" smd roundrect
		(at -13.35 2.9)
		(size 1.5 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.166667)
	)
	(pad "MP" smd roundrect
		(at 13.35 2.9)
		(size 1.5 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.166667)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S12B-PH-SM4-TB_1x12-1MP_P2.00mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
