(footprint "JST_PUD_B28B-PUDSS_2x14_P2.00mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "JST PUD series connector, B28B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator")
	(tags "connector JST PUD side entry")
	(property "Reference" "REF**"
		(at 13 -5.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "JST_PUD_B28B-PUDSS_2x14_P2.00mm_Vertical"
		(at 13 5.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 13 -3.2 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.208333)
	)
	(pad "2" thru_hole circle
		(at 0 2)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2 0)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2 2)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 4 0)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 4 2)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 6 0)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 6 2)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 8 0)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 8 2)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 10 0)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 10 2)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 12 0)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 12 2)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 14 0)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 14 2)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 16 0)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 16 2)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at 18 0)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at 18 2)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 20 0)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at 20 2)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole circle
		(at 22 0)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at 22 2)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 24 0)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "26" thru_hole circle
		(at 24 2)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole circle
		(at 26 0)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "28" thru_hole circle
		(at 26 2)
		(size 1.2 1.2)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PUD_B28B-PUDSS_2x14_P2.00mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
