(footprint "JST_VH_B4P-VH-FB-B_1x04_P3.96mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "JST VH series connector, B4P-VH-FB-B, shrouded (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf),  generated with kicad-footprint-generator")
	(tags "connector JST VH side entry")
	(property "Reference" "REF**"
		(at 5.94 -5.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "JST_VH_B4P-VH-FB-B_1x04_P3.96mm_Vertical"
		(at 5.94 6.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5.94 2.5 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -1.5 -3.4)
		(size 1.45 1.45)
		(drill 1.45)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.7 2.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.092593)
	)
	(pad "2" thru_hole circle
		(at 3.96 0)
		(size 2.7 2.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 7.92 0)
		(size 2.7 2.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 11.88 0)
		(size 2.7 2.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_VH_B4P-VH-FB-B_1x04_P3.96mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
