(footprint "JST_XA_S02B-XASK-1_1x02_P2.50mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "JST XA series connector, S02B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator")
	(tags "connector JST XA horizontal hook")
	(property "Reference" "REF**"
		(at 1.25 -4.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "JST_XA_S02B-XASK-1_1x02_P2.50mm_Horizontal"
		(at 1.25 10.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1.25 2.5 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole oval
		(at 1.25 6.5)
		(size 2.8 2)
		(drill oval 2.8 2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.147059)
	)
	(pad "2" thru_hole oval
		(at 2.5 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XA_S02B-XASK-1_1x02_P2.50mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
