(footprint "JST_XH_B16B-XH-A_1x16_P2.50mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "JST XH series connector, B16B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST XH side entry")
	(property "Reference" "REF**"
		(at 18.75 -3.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "JST_XH_B16B-XH-A_1x16_P2.50mm_Vertical"
		(at 18.75 4.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 18.75 2.7 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.147059)
	)
	(pad "2" thru_hole oval
		(at 2.5 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 5 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 7.5 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 10 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 12.5 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 15 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 17.5 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at 20 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at 22.5 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole oval
		(at 25 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole oval
		(at 27.5 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole oval
		(at 30 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole oval
		(at 32.5 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole oval
		(at 35 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole oval
		(at 37.5 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B16B-XH-A_1x16_P2.50mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
