(footprint "JST_XH_S3B-XH-SM4-TB_1x03-1MP_P2.50mm_Horizontal"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "JST XH series connector, S3B-XH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST XH horizontal")
	(property "Reference" "REF**"
		(at 0 -6.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "JST_XH_S3B-XH-SM4-TB_1x03-1MP_P2.50mm_Horizontal"
		(at 0 6.7 0)
		(layer "F.Fab")
	)
	(attr smd)
	(pad "1" smd roundrect
		(at -2.5 -3.25)
		(size 1.3 4.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.192308)
	)
	(pad "2" smd roundrect
		(at 0 -3.25)
		(size 1.3 4.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.192308)
	)
	(pad "3" smd roundrect
		(at 2.5 -3.25)
		(size 1.3 4.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.192308)
	)
	(pad "MP" smd roundrect
		(at -5.7 3.55)
		(size 1.8 3.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.138889)
	)
	(pad "MP" smd roundrect
		(at 5.7 3.55)
		(size 1.8 3.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.138889)
	)
	(fp_text user "${REFERENCE}"
		(at 0 1.5 0)
		(layer "F.Fab")
	)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_S3B-XH-SM4-TB_1x03-1MP_P2.50mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
