(footprint "JST_ZE_B02B-ZESK-1D_1x02_P1.50mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "JST ZE series connector, B02B-ZESK-1D, with boss (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator")
	(tags "connector JST ZE side entry boss")
	(property "Reference" "REF**"
		(at 0.75 -6.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "JST_ZE_B02B-ZESK-1D_1x02_P1.50mm_Vertical"
		(at 0.75 1.85 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0.75 -4.4 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -1.65 -3.8)
		(size 0.85 0.85)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole custom
		(at 0 0)
		(size 1.117157 1.117157)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.45 -0.225) (xy 0.45 0.625) (xy -0.45 0.625) (xy -0.45 -0.625) (xy 0.05 -0.625)
				)
				(width 0.5)
				(fill yes)
			)
		)
	)
	(pad "2" thru_hole oval
		(at 1.5 -2)
		(size 1.4 1.75)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_ZE_B02B-ZESK-1D_1x02_P1.50mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
