(footprint "JST_ZE_S16B-ZESK-2D_1x16_P1.50mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "JST ZE series connector, S16B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator")
	(tags "connector JST ZE top entry")
	(property "Reference" "REF**"
		(at 11.25 -2.08 0)
		(layer "F.SilkS")
	)
	(property "Value" "JST_ZE_S16B-ZESK-2D_1x16_P1.50mm_Horizontal"
		(at 11.25 8.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 11.25 3.45 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -1.55 1.85)
		(size 1.15 1.15)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 24.05 1.85)
		(size 1.15 1.15)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.4 1.75)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.178571)
	)
	(pad "2" thru_hole oval
		(at 1.5 3.7)
		(size 1.4 1.75)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 3 0)
		(size 1.4 1.75)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 4.5 3.7)
		(size 1.4 1.75)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 6 0)
		(size 1.4 1.75)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 7.5 3.7)
		(size 1.4 1.75)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 9 0)
		(size 1.4 1.75)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 10.5 3.7)
		(size 1.4 1.75)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at 12 0)
		(size 1.4 1.75)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at 13.5 3.7)
		(size 1.4 1.75)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole oval
		(at 15 0)
		(size 1.4 1.75)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole oval
		(at 16.5 3.7)
		(size 1.4 1.75)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole oval
		(at 18 0)
		(size 1.4 1.75)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole oval
		(at 19.5 3.7)
		(size 1.4 1.75)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole oval
		(at 21 0)
		(size 1.4 1.75)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole oval
		(at 22.5 3.7)
		(size 1.4 1.75)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_ZE_S16B-ZESK-2D_1x16_P1.50mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
