(footprint "JST_ZH_B12B-ZR_1x12_P1.50mm_Vertical"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "JST ZH series connector, B12B-ZR (http://www.jst-mfg.com/product/pdf/eng/eZH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST ZH vertical")
	(property "Reference" "REF**"
		(at 8.25 -2.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "JST_ZH_B12B-ZR_1x12_P1.50mm_Vertical"
		(at 8.25 3.4 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.03 1.73)
		(drill 0.73)
		(layers "*.Cu" "*.Mask")
		(roundrect_rratio 0.242718)
	)
	(pad "2" thru_hole oval
		(at 1.5 0)
		(size 1.03 1.73)
		(drill 0.73)
		(layers "*.Cu" "*.Mask")
	)
	(pad "3" thru_hole oval
		(at 3 0)
		(size 1.03 1.73)
		(drill 0.73)
		(layers "*.Cu" "*.Mask")
	)
	(pad "4" thru_hole oval
		(at 4.5 0)
		(size 1.03 1.73)
		(drill 0.73)
		(layers "*.Cu" "*.Mask")
	)
	(pad "5" thru_hole oval
		(at 6 0)
		(size 1.03 1.73)
		(drill 0.73)
		(layers "*.Cu" "*.Mask")
	)
	(pad "6" thru_hole oval
		(at 7.5 0)
		(size 1.03 1.73)
		(drill 0.73)
		(layers "*.Cu" "*.Mask")
	)
	(pad "7" thru_hole oval
		(at 9 0)
		(size 1.03 1.73)
		(drill 0.73)
		(layers "*.Cu" "*.Mask")
	)
	(pad "8" thru_hole oval
		(at 10.5 0)
		(size 1.03 1.73)
		(drill 0.73)
		(layers "*.Cu" "*.Mask")
	)
	(pad "9" thru_hole oval
		(at 12 0)
		(size 1.03 1.73)
		(drill 0.73)
		(layers "*.Cu" "*.Mask")
	)
	(pad "10" thru_hole oval
		(at 13.5 0)
		(size 1.03 1.73)
		(drill 0.73)
		(layers "*.Cu" "*.Mask")
	)
	(pad "11" thru_hole oval
		(at 15 0)
		(size 1.03 1.73)
		(drill 0.73)
		(layers "*.Cu" "*.Mask")
	)
	(pad "12" thru_hole oval
		(at 16.5 0)
		(size 1.03 1.73)
		(drill 0.73)
		(layers "*.Cu" "*.Mask")
	)
	(fp_text user "${REFERENCE}"
		(at 8.25 1.5 0)
		(layer "F.Fab")
	)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_ZH_B12B-ZR_1x12_P1.50mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
