(footprint "JST_ZH_B6B-ZR-SM4-TF_1x06-1MP_P1.50mm_Vertical"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "JST ZH series connector, B6B-ZR-SM4-TF (http://www.jst-mfg.com/product/pdf/eng/eZH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST ZH vertical")
	(property "Reference" "REF**"
		(at 0 -4.35 0)
		(layer "F.SilkS")
	)
	(property "Value" "JST_ZH_B6B-ZR-SM4-TF_1x06-1MP_P1.50mm_Vertical"
		(at 0 3.75 0)
		(layer "F.Fab")
	)
	(attr smd)
	(pad "1" smd roundrect
		(at -3.75 0.7)
		(size 0.7 3.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.25 0.7)
		(size 0.7 3.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -0.75 0.7)
		(size 0.7 3.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0.75 0.7)
		(size 0.7 3.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 2.25 0.7)
		(size 0.7 3.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 3.75 0.7)
		(size 0.7 3.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP" smd roundrect
		(at -5.8 -1.4)
		(size 1.5 2.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.166667)
	)
	(pad "MP" smd roundrect
		(at 5.8 -1.4)
		(size 1.5 2.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.166667)
	)
	(fp_text user "${REFERENCE}"
		(at 0 -1.5 0)
		(layer "F.Fab")
	)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_ZH_B6B-ZR-SM4-TF_1x06-1MP_P1.50mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
