(footprint "JST_ZH_S11B-ZR-SM4A-TF_1x11-1MP_P1.50mm_Horizontal"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "JST ZH series connector, S11B-ZR-SM4A-TF (http://www.jst-mfg.com/product/pdf/eng/eZH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST ZH horizontal")
	(property "Reference" "REF**"
		(at 0 -4.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "JST_ZH_S11B-ZR-SM4A-TF_1x11-1MP_P1.50mm_Horizontal"
		(at 0 5.2 0)
		(layer "F.Fab")
	)
	(attr smd)
	(pad "1" smd roundrect
		(at -7.5 -1.65)
		(size 0.7 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -6 -1.65)
		(size 0.7 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -4.5 -1.65)
		(size 0.7 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3 -1.65)
		(size 0.7 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.5 -1.65)
		(size 0.7 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 0 -1.65)
		(size 0.7 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 1.5 -1.65)
		(size 0.7 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 3 -1.65)
		(size 0.7 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 4.5 -1.65)
		(size 0.7 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 6 -1.65)
		(size 0.7 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 7.5 -1.65)
		(size 0.7 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP" smd roundrect
		(at -9.45 2.05)
		(size 1.1 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "MP" smd roundrect
		(at 9.45 2.05)
		(size 1.1 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_ZH_S11B-ZR-SM4A-TF_1x11-1MP_P1.50mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
