(footprint "Molex_CLIK-Mate_502494-1570_1x15-1MP_P2.00mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex CLIK-Mate series connector, 502494-1570 (http://www.molex.com/pdm_docs/sd/5024940270_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex CLIK-Mate top entry")
	(property "Reference" "REF**"
		(at 0 -5.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_CLIK-Mate_502494-1570_1x15-1MP_P2.00mm_Horizontal"
		(at 0 6.35 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0.38 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -14 -2.5)
		(size 1 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -12 -2.5)
		(size 1 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -10 -2.5)
		(size 1 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -8 -2.5)
		(size 1 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -6 -2.5)
		(size 1 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -4 -2.5)
		(size 1 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -2 -2.5)
		(size 1 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 0 -2.5)
		(size 1 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 2 -2.5)
		(size 1 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 4 -2.5)
		(size 1 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 6 -2.5)
		(size 1 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 8 -2.5)
		(size 1 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 10 -2.5)
		(size 1 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 12 -2.5)
		(size 1 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 14 -2.5)
		(size 1 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP" smd roundrect
		(at -16.35 1.95)
		(size 1.8 3.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.138889)
	)
	(pad "MP" smd roundrect
		(at 16.35 1.95)
		(size 1.8 3.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.138889)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_CLIK-Mate_502494-1570_1x15-1MP_P2.00mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
