(footprint "Molex_Mega-Fit_76829-0104_2x02_P5.70mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex Mega-Fit Power Connectors, 76829-0104 (compatible alternatives: 172065-0204, 172065-0304), 2 Pins per row (http://www.molex.com/pdm_docs/sd/768290102_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex Mega-Fit side entry")
	(property "Reference" "REF**"
		(at 2.85 -4.51 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_Mega-Fit_76829-0104_2x02_P5.70mm_Vertical"
		(at 2.85 11.92 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.85 -2.61 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 8.18 8.47)
		(size 1.8 1.8)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 3.7 3.7)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.067568)
	)
	(pad "2" thru_hole circle
		(at 5.7 0)
		(size 3.7 3.7)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 5.7)
		(size 3.7 3.7)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 5.7 5.7)
		(size 3.7 3.7)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Mega-Fit_76829-0104_2x02_P5.70mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
