(footprint "Molex_Micro-Fit_3.0_43045-0210_2x01-1MP_P3.00mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex Micro-Fit 3.0 Connector System, 43045-0210 (compatible alternatives: 43045-0211, 43045-0209), 1 Pins per row (http://www.molex.com/pdm_docs/sd/430450210_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex Micro-Fit_3.0 top entry")
	(property "Reference" "REF**"
		(at 0 -13.58 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_Micro-Fit_3.0_43045-0210_2x01-1MP_P3.00mm_Horizontal"
		(at 0 4.98 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -11.68 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 0 -2.315)
		(size 1.27 2.92)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0 2.315)
		(size 1.27 2.92)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at -3.885 -7.785)
		(size 3.43 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at 3.885 -7.785)
		(size 3.43 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Micro-Fit_3.0_43045-0210_2x01-1MP_P3.00mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
