(footprint "Molex_Micro-Fit_3.0_43650-0415_1x04_P3.00mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex Micro-Fit 3.0 Connector System, 43650-0415 (compatible alternatives: 43650-0416, 43650-0417), 4 Pins per row (http://www.molex.com/pdm_docs/sd/436500215_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex Micro-Fit_3.0 vertical")
	(property "Reference" "REF**"
		(at 4.5 -3.67 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_Micro-Fit_3.0_43650-0415_1x04_P3.00mm_Vertical"
		(at 4.5 4.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 4.5 1.2 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -3 -1.96)
		(size 1.27 1.27)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 12 -1.96)
		(size 1.27 1.27)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.5 2.02)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.166667)
	)
	(pad "2" thru_hole oval
		(at 3 0)
		(size 1.5 2.02)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 6 0)
		(size 1.5 2.02)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 9 0)
		(size 1.5 2.02)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Micro-Fit_3.0_43650-0415_1x04_P3.00mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
