(footprint "Molex_Micro-Fit_3.0_43650-0921_1x09_P3.00mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex Micro-Fit 3.0 Connector System, 43650-0921 (compatible alternatives: 43650-0922, 43650-0923), 9 Pins per row (https://www.molex.com/pdm_docs/sd/436500221_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex Micro-Fit_3.0 vertical")
	(property "Reference" "REF**"
		(at 0 -3.38 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_Micro-Fit_3.0_43650-0921_1x09_P3.00mm_Vertical"
		(at 0 5.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 1.48 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -14.15 -0.285)
		(size 2.41 2.41)
		(drill 2.41)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 14.15 -0.285)
		(size 2.41 2.41)
		(drill 2.41)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -12 3.135)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -9 3.135)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -6 3.135)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3 3.135)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 0 3.135)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 3 3.135)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 6 3.135)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 9 3.135)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 12 3.135)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Micro-Fit_3.0_43650-0921_1x09_P3.00mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
