(footprint "Molex_MicroClasp_55935-1110_1x11_P2.00mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex MicroClasp Wire-to-Board System, 55935-1110, with PCB locator, 11 Pins (http://www.molex.com/pdm_docs/sd/559350210_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex MicroClasp horizontal")
	(property "Reference" "REF**"
		(at 10 -3.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_MicroClasp_55935-1110_1x11_P2.00mm_Horizontal"
		(at 10 10.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 10 8.5 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2 2.4)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 22 2.4)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.2 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.208333)
	)
	(pad "2" thru_hole oval
		(at 2 0)
		(size 1.2 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 4 0)
		(size 1.2 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 6 0)
		(size 1.2 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 8 0)
		(size 1.2 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 10 0)
		(size 1.2 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 12 0)
		(size 1.2 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 14 0)
		(size 1.2 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at 16 0)
		(size 1.2 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at 18 0)
		(size 1.2 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole oval
		(at 20 0)
		(size 1.2 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_MicroClasp_55935-1110_1x11_P2.00mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
