(footprint "Molex_Mini-Fit_Jr_5566-02A2_2x01_P4.20mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex Mini-Fit Jr. Power Connectors, old mpn/engineering number: 5566-02A2, example for new mpn: 39-28-902x, 1 Pins per row, Mounting: Snap-in Plastic Peg PCB Lock (http://www.molex.com/pdm_docs/sd/039289068_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex Mini-Fit_Jr side entryplastic_peg")
	(property "Reference" "REF**"
		(at 0 -3.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_Mini-Fit_Jr_5566-02A2_2x01_P4.20mm_Vertical"
		(at 0 9.95 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 -1.55 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -4.7 5.04)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 4.7 5.04)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.7 3.3)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.092593)
	)
	(pad "2" thru_hole oval
		(at 0 5.5)
		(size 2.7 3.3)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Mini-Fit_Jr_5566-02A2_2x01_P4.20mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
