(footprint "Molex_Mini-Fit_Jr_5569-02A1_2x01_P4.20mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex Mini-Fit Jr. Power Connectors, old mpn/engineering number: 5569-02A1, example for new mpn: 39-29-4029, 1 Pins per row, Mounting: PCB Mounting Flange (http://www.molex.com/pdm_docs/sd/039291047_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex Mini-Fit_Jr top entryscrew_flange")
	(property "Reference" "REF**"
		(at 0 -15.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_Mini-Fit_Jr_5569-02A1_2x01_P4.20mm_Horizontal"
		(at 0 8.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 -13.2 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -4.5 -4.2)
		(size 3.2 3.2)
		(drill 3.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 4.5 -4.2)
		(size 3.2 3.2)
		(drill 3.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.7 3.7)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.092593)
	)
	(pad "2" thru_hole oval
		(at 0 5.5)
		(size 2.7 3.7)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Mini-Fit_Jr_5569-02A1_2x01_P4.20mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
